



Key Features

It has tripod thread for using of tripod.

|  |  |
| --- | --- |
| Type | : Multiple coated glass optics |
| Magnification | : 8x |
| Field of view | : 6.5° |
| Diopter adjustment | : ±5 |
| Laser protection for observer | : Laser wavelength: 1535nm |
| Minimum measuring range | : 10meters |
| Maximum measuring range | : 5500meters |
| Accuracy | : ±1m |
| Laser classification | : Laser class 1 |
| Display | : OLED display with reticle |
| Power source | : Rechargeable battery |
| Battery lifetime | : >3,000 measurements (per battery set, at 20oC  operating temperature) |
| Standards | : MIL-STD-810F |
| Water resistance | : IP67(30 minutes, 1m) |
| Operating temperature | : -30oC~+60oC |
| Storage temperature | : -40oC~+80oC |
| Provided with | : Tripod |
|  | \*Extended length: 1670mm |
|  | \*Folder length:620mm |
|  | \*Weight: 1.87kg |
| Accessories | : Standard transport bag and operating manual in  English/Chinese & one charger. |